{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Costabid"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Costabid","index":0,"n_rows":24,"n_cols":6,"rows_kept":24,"cut":false,"hidden":false,"merged":[[7,0,7,2],[7,3,7,5],[1,1,1,5],[2,1,2,5],[3,1,3,5],[6,0,6,5],[5,0,5,5]]}
[]
[null,"CIPET IPT-CHENNAI"]
[null,"T.V.K. Industrial Estate,"]
[null,"Guindy, Chennai - 600 032."]
[null,null,null,null,null,"Annexure -I"]
["PRICE SCHEDULE"]
["Name of Work :- Water Proofing - Repair work at the terrace area of CAD/CAM/CAE department and Design department at CIPET: IPT, CHENNAI"]
["Name of the Bidder"]
["S No","Description","Qty","Units","Unit Price  \n(Rs.)\n","Amount In Rs."]
["I","Area - CAD/CAM/CAE  – Dept.\nApplication of Polymer Reinforced bitumen membrane [ A high performance water proofing membrane made of polymer reinforced bitumen of 3mm thickness]"]
["i)","Existing, worn out Tar sheet removal.",6232.44,"SQ.FT",null,{"$f":"C11*E11","v":0.0}]
["ii)","New Tar Sheet Laying charges",6232.44,"SQ.FT",null,{"$f":"C12*E12","v":0.0}]
["II","Area - Design – Dept.\nApplication of Polymer Reinforced bitumen membrane [ A high performance water proofing membrane made of polymer reinforced bitumen of 3mm thickness]\n"]
["i)","Existing, worn out Tar sheet removal.",4225.0,"SQ.FT",null,{"$f":"C14*E14","v":0.0}]
["ii)","New Tar Sheet",4225.0,"SQ.FT",null,{"$f":"C15*E15","v":0.0}]
[]
[null,"Total",null,null,null,{"$f":"SUM(F10:F16)","v":0.0}]
[null,"GST 18%",null,null,null,{"$f":"F17*18%","v":0.0}]
[]
[null,"Grand Total",null,null,null,{"$f":"SUM(F16:F19)","v":0.0}]
[]
[]
["Date ",null,null,null,"Signature Bidder"]
["Place"]