

CIPET: CSTS/Dehradun/Purchase/Tender/2022-23/01 Dated:21.06.2022

**TENDER DOCUMENT**

**FOR**

**Supply & Installation of Uniformity of Emission Rate Apparatus for Emitting pipes as per IS 13488**

Deputy Director & Incharge

CENTRAL INSTITUTE OF PETROCHEMICALS ENGINEERING AND TECHNOLOGY

CIPET: CENTER FOR SKILLING AND TECHNICAL SUPPORT (CSTS)

(Department of Chemicals & Petrochemicals, Ministry of Chemicals & Fertilizers, Govt. of India)

Haridwar Road, Post-Bhaniyawala, Doiwala, Dehradun – 248140 (U.K.)

Telephone-01352695075, Email:Dehradun@cipet.gov.in

Website: [www.cipet.gov.in](http://www.cipet.gov.in)

CIPET: CSTS/Dehradun/Purchase/Tender/2022-23/01 Dated:21.06.2022

**TENDER NOTICE**

CIPET: CSTS Dehradun invites Tender for Supply & Installation of Uniformity of Emission Rate Apparatus for Emitting pipes as per IS 13488

|  |  |
| --- | --- |
| **S.No.** | **Name of work** |
| **1.** | **Supply and Installation of Uniformity of Emission Rate Apparatus for Emitting pipes as per IS 13488** |

1. Interested and eligible Suppliers / providers are to submit a hard copy of the quotation along with requisite documents duly sealed and signed to the Deputy Director & Incharge, CIPET: CSTS, Dehradun, Haridwar Road, Post-Bhaniyawala, Doiwala, Dehradun – 248140 (U.K) on or before  **04.07.2022** before **5 PM**
2. The Suppliers are required to submit two Envelopes marking as **Technical Bid and Financial Bid** by SPEED POST/REGISTERED POST/ Hand only to the CIPET: CSTS, Dehradun, (U.K.) India-248140.
3. The Supplier which qualifies the Technical Opening shall only be considered for financial opening. CIPET: CSTS, Dehradun reserves the right to reject any or all the Tenders received without assigning any reason(s) thereof.

Deputy Director & Incharge

CIPET: CSTS, Dehradun

**Essential Requirements for the Tender**

1. **Minimum Eligibility of the suppliers**
2. Should have minimum turnover of Rs. 10 lakh per year during each of the last two years (valid and certified proof has to be attached);
3. Should not have been blacklisted by the Depts./Ministries of the Govt. of India/PSUs Etc. (declaration has to be submitted in the format as Annexure -1).
4. Should meet all the Technical Specifications as attached in Annexure II
5. **Tender Prices**
6. The rates/ prices should be quoted in Indian Rupees (INR) only in words as well as figures. Taxes, if any, should be indicated separately.
7. Prices should be quoted FOR CIPET: CSTS, Dehradun including Installation Charge.( No additional freight charges will be paid)
8. **Submission of Tender**
9. **Sealing, Marking & Submission**
10. **Envelope No.1 marked as Technical Bid** shall contain, Declaration (Annexure I), Turnover for the last two years and Technical Specifications of Apparatus.
11. **Envelope No.2** shall contain the Price of the Apparatus.

All the above envelopes shall bear the Name of the Bid *viz*.

**‘Supply & Installation of Uniformity of Emission Rate Apparatus for Emitting pipes as per IS 13488’**

1. **Award of Contract and Mode of Payment**
2. Delivery within 45 days from the date of Purchase Order
3. The Performance Guarantee equivalent to the amount of 5% of total contract price, having a validity of 29 months.
4. Payment against submission of Bill/Invoice shall be released only after successful Installation of the Apparatus.
5. Payment will be made directly to the Supplier through A/c Payee Cheque/NEFT only.
6. No request for other mode of payment will be entertained. No advance payment will be made in any case

.

**Annexure - I**

**DECLARATION**

(TO BE TYPED ON A LETTER HEAD OF THE COMPANY/ FIRM)

To

The Deputy Director & Incharge

CIPET: CSTS

Haridwar Road, Post-Bhaniyawala, Doiwala,

Dehradun – 248140 (U.K)

Dear Sir,

1. We have carefully read and understood all the terms and conditions of the Tender and agree to abide by the terms and conditions.
2. I/We also confirm that in the event of my/our offer being accepted, I/we hereby undertake to furnish EMD, as applicable, in the form of Demand Draft.
3. I/We further undertake that none of the Proprietor/Partners/Directors of the firm was or is Proprietor or Partner or Director of any firm with whom the Government have blacklisted/banned / suspended business dealing. I/We further undertake to report to the CIPET: CSTS, Dehradun immediately after we are informed but in any case not later than 15 days, if any firm in which Proprietor /Partners/Directors are Proprietor or Partner or Director of such a firm which is blacklisted/banned/suspended in future during the currency of the Contract with you. We have no objection, if enquiries are made about the work listed by us.

Yours faithfully,

Place:

Date:

Signature of authorized person

Full Name & Designation:

Company’s Seal:

**Note: The above declaration, duly signed and sealed by the authorized signatory of the company, should be enclosed with EOI document.**

**Annexure II**

1. **Technical Specifications**
2. Test Specimen nos. 25 with max spacing of 600 mm with a provision of NABL Calibrated Digital Timer with accuracy, 0.1 sec
3. Material Construction: Stainless Steel
4. NABL Calibrated Measuring Cylinders of Min, 600 ml (Transparent Plastic) – 25 nos.
5. Water Tank Capacity: 50 Litres, Min
6. Pressure Range: 0-5 kg/cm2 ; Resolution: 0.05 kg/cm2
7. Machine should comply to IS 13488
8. NABL Calibration certificates are to be provided for all parameters